Revision history of Board changes:

|  |  |  |
| --- | --- | --- |
| Board Revision | Details of changes | Device version |
| IWRL6432FSP EVM Rev A | Baseline | ES1.0 |
| IWRL6432FSP EVM Rev B | * Changed type number of 1.2VDC and 1.8VDC buck * Added pull down resistor to 1.2VDC and 1.8VDC buck’s MODE pin, and removed pull up circuit * Un-populate resistor and capacitor on GPADC1 and GPADC2 circuit * Changed pull up resistor to 2Mohm on TX, RX, I2C\_SCL and I2C\_SDA pins * Removed filter capacitor on RADAR\_1V8, RADAR\_1V2 and RADAR\_1P2\_RF tracks * Changed bead on RADAR\_1V8, RADAR\_1V2 and RADAR\_1P2\_RF tracks to 0ohm * Removed 33ohm on signal tracks of flash * Changed pull up resistor to 2Mohm on signal tracks of flash | ES1.0 |
|  |  |  |
|  |  |  |